# sustainable Transport Healthcare Prescriptive pathway

### Credit 17B

### Design Review Submission [ ]  As Built Submission [ ]

|  |  |  |  |
| --- | --- | --- | --- |
| Total Points available: | 10 | Points claimed: | [#] |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Criterion Name | Points Available | Points Claimed |
| **17B.1** | **Access by public transport** | 4 | [#] |
| **17B.2** | **Reduced car parking provision** | 1 | [ ]  |
| **17B.3** | **Low emission vehicle infrastructure** | 2 | [ ]  |
| **17B.4** | **Active transport facilities** | 2 | [ ]  |
| **17B.5** | **Walkable neighbourhood** | 1 | [ ]  |

## Project-specific technical questions (formerly tcs and cirs)

|  |
| --- |
| There are no project-specific Technical Questions for this credit. |[ ]
| There are project-specific Technical Questions for this credit and all responses received from the NZGBC are attached. |[ ]

|  |
| --- |
| **Summary of Expected Building Occupant Numbers** |
|  | Expected Numbers |
| Regular Occupants | [x] |
| Visitors | [x] |
| Staff | [x] |
| Peak Occupancy | [x] |
| [other occupant type] | [x] |

### 17B General

### 17B.1A Access by Public Transport: deemed to satisfy

|  |  |
| --- | --- |
| Project postcode | [x] |

### 17B.1B Access by Public Transport: transport calculator

|  |  |
| --- | --- |
| Number of points awarded in the Transport Calculator | [x] |
| Points Claimed | [x] |

[Insert hyperlinks to Green Star Access by Public Transport Calculator]

### 17B.2 Reduced Car Parking Provision

|  |  |
| --- | --- |
| Accessibility Rating (determined by criterion 17D.1) | [x] |
| Maximum car parking to occupant ratio | [x] |
| No car parking is provided | [ ]  |

|  |
| --- |
| **Car Carking Provisions** |
| **Space Use Type** | **Number of Occupants** | **Maximum Car Parking Ratio** | **Max Spaces Permitted** | **Spaces Provided** | **Points Claimed** |
| [space use] | [x] | [1 to 30] | [x] | [x] | [0.5, 1] |
| [space use] | [x] | [1 to 30] | [x] | [x] |  |
| [space use] | [x] | [1 to 30] | [x] | [x] |  |

Identify where this information can be found within the supporting documentation provided.

|  |  |
| --- | --- |
| **Supporting Documentation** (Name / title / description of document) | **Reference**(Page no. or section) |
| [####] | [####] |
| [####] | [####] |

### 17B.3 Low Emission Vehicle Infrastructure

|  |  |  |
| --- | --- | --- |
| **Low Emission Vehicle Infrastructure** |  | **Points Available** |
| 15% of parking is designated for fuel efficient vehicles, with a maximum of 5% for motorcycle parking. | [ ]  | 1 |
| 5% of total parking provided is designated for use by electric vehicles and charging infrastructure is provided for each space. | [ ]  | 1 |

Provide a description of how the project meets the requirements for low emission vehicle infrastructure

Identify where this information can be found within the supporting documentation provided.

|  |  |
| --- | --- |
| **Supporting Documentation** (Name / title / description of document) | **Reference**(Page no. or section) |
| [####] | [####] |
| [####] | [####] |

### 17B.4 Active Transport Facilities

|  |  |  |
| --- | --- | --- |
| **Active Transport Facilities** |  | **Points Available** |
| Active Transport Facilities (where required) have been provided to regular building occupants. | [ ]  | 1 |
| Active Transport Facilities have been provided to building visitors. | [ ]  | 1 |

Provide a description of secure bicycle parking spaces and end of trip facilities.

|  |
| --- |
| **Summary of Cycle Facilities** |
| **Secure Cycle Facilities for regular occupants** |
| Credit Requirement | [x] | Provided | [ ]  |
| **Visitor cycle parking** |
| Credit Requirement | [x] | Provided | [ ]  |
| **End of Trip Facilities for Staff**  |
| Credit Requirement | [x] | Provided | [ ]  |

Identify where this information can be found within the supporting documentation provided.

|  |  |
| --- | --- |
| **Supporting Documentation** (Name / title / description of document) | **Reference**(Page no. or section) |
| [####] | [####] |
| [####] | [####] |

### 17B.5 walkable neighbourhoods

|  |  |
| --- | --- |
| Project Walkscore. | [x] |
| At least six amenities (for projects located outside a designated central business district, commercial or retail zone) or at least eight amenities (for projects located within a designated central business district, commercial or retail zon) are within 400m of the development. | [ ]  |

Identify where Walkscore report or a summary of the number of amenities within the relevant distance to the site can be found within the supporting documentation provided.

|  |  |
| --- | --- |
| **Supporting Documentation** (Name / title / description of document) | **Reference**(Page no. or section) |
| [####] | [####] |
| [####] | [####] |

## DISCUSSION

Outline any issues you would like to highlight and clarify with the Certified Assessor(s).

## DECLARATION

I confirm that the information provided in this document is truthful and accurate at the time of completion.

Provide author details, including name, position and email address:

[Date]

 ––– **Report end** –––